{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":10,"n_cols":4,"rows_kept":10,"merged":[[0,0,0,4],[1,3,1,4],[2,3,2,4],[3,3,3,4],[4,3,4,4],[5,3,5,4],[6,3,6,4],[7,3,7,4],[8,3,8,4],[9,3,9,4]],"flags":["formulas_cached_only"]}
["建筑装饰样板间装修工程清单"]
["序号","设备名称","数量","技术参数"]
[1,"装饰样板间\n（两室两厅双卫）其中一卫为明装下列洁具设备\n","100平","家装样板间基础装修+软装:1、装饰样板间主要作用是展示装饰设计的主流装饰装修风格如中式、欧式、日韩、东南亚、现代简约、乡村田园中的几种、混搭等风格及其体现元素，展示装饰效果，实际感受设计方案的尺度、工艺水准、材料质感、施工质量，样板制度是对工程项目的进度、质量、成本乃至效果都有很大的帮助，也是装修效果的参照实例；2、技术要求如下，作为学校学习使用的装饰样板间，考虑到装饰风格的多样性，和对教学效果最有益，各个卧室、客厅、书房（起居室）餐厅、厨房、卫生间等尽量按不同风格进行设计，3、其中一卫需明装常见给排水专业所需的卫生洁具设备，同时各个房间内硬装部分体现常见地面装饰材料各种地砖、地板成品铺装，常见墙面材料大白乳胶漆硅藻泥、壁纸墙布、各种墙面砖、饰面板的涂饰裱糊与安装，常见石膏吊顶、各种顶棚构造如铝扣板铝塑板等成品顶棚；4、各房间必备的卧室床榻及其窗帘床上用品、书桌椅、地毯、电灯台灯等电气设备与排线插座等，5、客厅阳台所需沙发茶几电视柜背景墙绿植、墙上背景工艺品脚踏，餐厅所需餐桌椅餐具灯具酒柜，厨房所需灶台及台板、厨房电气炊具工具、橱柜等，卫生间所需洗衣机热水器、洗漱用具正冠理容用具，以及其他必备家庭生活用品、暖气地热等取暖用具等，所有部分要求易清洁。"]
[2,"展示橱窗","按延米算室内15米","走廊或专业实训室内墙，展示学生作品成果和系部专业发展历程与成果，材料要求：铝塑板用来贴面，木方和大芯板用来做柜体框架，最少18厚，九厘板就是用来做背板的，面可以用墙纸，也可以上乳胶漆，图案待定，橱窗玻璃用10MM钢化玻璃，安全第一！不锈钢外框装饰条及密封胶、万能胶、腻子等辅料。落地支架或固定在墙壁上，led灯光照明系统，橱窗开启开关，方便更换展品，展示架格设计美观合理，可参考博古架和商品柜台展架，所有外部面层要求易清洁"]
[2,"玻璃钢水箱",1,"储水箱500*500SMC水箱，附带管线附件，自动上水、停水控制"]
[3,"热水器",1,"最大容积: 60L;     尺寸: φ463X693mm功率2000W，附带连接附件并安装好"]
[4,"花洒",2,"单把双控，顶喷，手喷，洗衣机水龙头，附带管线附件"]
[5,"洗手盆",2,"柱式手盆600*400，附带管线附件含单把双控水龙头\n"]
[6,"坐便器",2,"冲水量：3/4.5L；喷射虹吸式充水；缓冲盖板，附带管线附件，另小便器、大便器（自带冲水水箱）各一个"]
[7,"暖气散热器",2,"铝合金6柱1800*500，10柱600*1000，附带管线附件并连接好"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}